time, s

raw data bandpass filtered (200-1000 Hz) tapered to zero (10 ms window)